Remote processing – microprocessor that takes measurements and sends raw data to central control unit which does all the processing

* Much cheaper
* Relies on internet connectivity – unlikely to be an issue

Direct processing using raspberry pi and compute stick, less need to transfer large amounts of data